e – read a register

E – write a register

U – soft-start the LT8722

u – stop the 8722 switching

D- output zero volts on the output voltage.

V - output a floating point voltage.

For example

V1.000001

V-2.02

V4.5000000000000000

V3.2